|  |  |  |
| --- | --- | --- |
|  |  | **Estimated Price USD$** |
| **Startup/Commissioning Parts:** | Startup/commissioning parts are recommended to be available on site for immediate use during commissioning. Startup/commissioning parts typically include the following: spare fitting kit, hand tool kit, one (1) set of lube and fuel filtration elements, gaskets, O-rings, other sealing media, and a selection of electrical components with usage during normal startup and commissioning. | **$23,487.18** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Part Description** | **Recommended Qty** | **Unit Price** | **Ext Price** |
| **STARTUP/COMMISSIONING PARTS** |  |  |  |
| SEALANT, PIPE, PTFE | 1 |  |  |
| LAMP, LED, RED,28 VDC | 2 |  |  |
| INDICATOR, LIGHTED, YELLOW | 1 |  |  |
| INDICATOR, LIGHTED, WHITE | 10 |  |  |
| INDICATOR,LIGHTED,GREEN | 2 |  |  |
| GASKET,SPIRAL,2.0,CL300,RF | 2 |  |  |
| GASKET,SPIRAL,1.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,2.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,3.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,4.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,2.0,CL300,RF,304 | 2 |  |  |
| GASKET,0.375 OD,PFTE,JOINT | 1 |  |  |
| SEAL,LIP | 1 |  |  |
| HOLDER,FUSE | 10 |  |  |
| FUSE,2 A | 2 |  |  |
| FUSE,5 A | 2 |  |  |
| FUSE,10 A | 6 |  |  |
| FUSE,20 A | 2 |  |  |
| FUSE,30 A | 2 |  |  |
| CONNECTOR | 2 |  |  |
| O-RING,NON-STD,31.625 ID,VITON | 1 |  |  |
| SENSOR,SPEED,ACTIVE | 1 |  |  |
| KIT,ELEMENT,CARTRIDGE,PLEATED | 1 |  |  |
| RELAY,DPDT,8 A | 17 |  |  |
| SEAL,EXTRUSION | 1 |  |  |
| KIT,ELEMENT,FILTER,LUBE OIL | 2 |  |  |
| INDICATOR,LIGHTED | 1 |  |  |
| KIT,ELEMENT,FILTER | 2 |  |  |
| SEAL,METALLIC | 1 |  |  |
| SOCKET,RELAY,24 VDC,10 A | 1 |  |  |
| ELEMENT,BARRIER,CELLULOSE | 1 |  |  |
| SET,BOLT,SHEAR | 1 |  |  |
| ADHESIVE,THREADLOCK | 2 |  |  |
| BOLT,HEX,0.375-16 X 1.0 IN,B7 | 20 |  |  |
| CABLE,IGNITION,84.0 IN | 1 |  |  |
| GROMMET,0.965 OD | 1 |  |  |
| GROMMET,0.965 OD | 1 |  |  |
| GASKET, INJECTOR | 12 |  |  |
| GASKET,8.8 ID,10.66 OD,0.06 IN | 1 |  |  |
| GASKET X 2.71IN,.062,BLUE-GARD | 1 |  |  |
| PACKING,OIL DRAIN | 6 |  |  |
| GASKET,5.62 X 5.62IN,.030 | 3 |  |  |
| GASKET,3.32 ID,3.68 OD,0.049 | 5 |  |  |
| KIT,ELEMENT,FILTER,LUBE OIL | 1 |  |  |
| KIT,ELEMENT,FUEL,LUBE OIL,8.2 | 1 |  |  |
| SENSOR,SPEED,PASSIVE | 1 |  |  |
| GASKET,1.471 ID,1.754 OD,0.150 | 1 |  |  |
| TAPE,FOAM | 50 |  |  |
| SEALANT,PIPE,PUTTY | 1 |  |  |
| BULB FLUOR BI-PIN TUBE 36W | 2 |  |  |
| GASKET,42.25 ID,53 OD | 1 |  |  |
| O-RING,SAE 015,VITON | 25 |  |  |
| O-RING,SAE 214,1.0 ID,VITON | 25 |  |  |
| O-RING,SAE 227,2.125 ID,VITON | 10 |  |  |
| O-RING,SAE 158,4.75 ID,VITON | 6 |  |  |
| GASKET,0.77 ID,METALLIC,SPARK | 25 |  |  |
| SPARK PLUG | 2 |  |  |
| O-RING,SAE 166,6.75 ID,VITON | 4 |  |  |
| O-RING,SAE 117,0.8125 ID,VITON | 25 |  |  |
| O-RING,SAE 225,1.875 ID,VITON | 15 |  |  |
| O-RING,SAE 222,1.5 ID,VITON | 25 |  |  |
| O-RING,SAE 932,2.337 ID,VITON | 8 |  |  |
| O-RING,SAE 122,1.125 ID,VITON | 25 |  |  |
| O-RING,SAE 924,1.72 ID,VITON | 12 |  |  |
| LAMP,INCANDESCENT,CLEAR,28 VDC | 4 |  |  |
| SEAL,THREADED,0.625 ID,1.1875 | 8 |  |  |
| RESISTOR,0.25 W,10000 OHM | 25 |  |  |
| SEAL,METALLIC | 4 |  |  |
| WIRE,SAFETY,0.032 IN,302/304 | 1 |  |  |
| O-RING,SAE 224,1.75 ID,VITON | 14 |  |  |
| SEAL,THREADED,0.375 ID,0.75 OD | 10 |  |  |
| O-RING,SAE 137,VITON | 6 |  |  |
| SEAL,THREADED,0.759 ID,1.023 | 1 |  |  |
| BLOCK,MOUNTING,BARRIER SYS | 12 |  |  |
| SEAL, METALLIC 1/4'' SAE O-RNG | 1 |  |  |
| SEAL,METALLIC | 1 |  |  |
| SEAL,METALLIC | 1 |  |  |
| GASKET 6'' 150# FULL FACE | 1 |  |  |
| SEALANT | 3 |  |  |
| KIT,TOOL,HAND | 1 |  |  |
| TOOL,REPLACEMENT FITTINGS | 1 |  |  |
| **Subtotal (STARTUP/COMMISSIONING PARTS)** |  |  | **$23,487.18** |