Scope of Delivery 
for delivery of the GENSET 4500 or 4300
based on the MWM TCG 2032 V16 (B) 50Hz gas engine
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Schematic Process Flow Chart
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Scope of supply


Overview


	Number
	Title

	Genset

	Engine Parts

	1
	Engine configuration

	1
	Basic parts

	1
	Exhaust gas system

	1
	Exhaust expansion joint

	1
	Exhaust turbo charger

	1
	Cooling system

	1
	Torsional vibration damper

	1
	Fly wheel

	1
	Starter equipment

	1
	Engine Mounting

	1
	Speed and load regulation

	1
	Ignition device

	1
	Gas mixer

	1
	TEM Engine monitoring and control

	1
	Primer and Topcoat Engine - Primer

	1
	Conservation

	1
	without spare parts for commissioning

	Mixtrure Piping

	1
	Gas mixture pipe without compressor cooling

	Lubrication System

	1
	Lube oil system

	Genset Parts

	1
	Genset defintion

	1
	Generator - Marelli MJH 800 MC6 / TDPS TD 145

	1
	Base frame without integrated oil tank

	1
	Elastic genset mounting

	1
	Elastic coupling

	1
	Fasteners

	1
	Crankcase ventilation

	1
	Piping (plain bearing)

	1
	Coolant preheat V

	1
	Coolant expansion joints water / oil

	1
	Pre Lubrication Genset - 400 / 690 / 460 V

	1
	Additional parts for lubrication system 230 V

	1
	Air filter, lateral air supply, with console

	1
	Caps for gas connection




	1
	Compressed air control train

	Primer and Topcoat for Genset

	1
	Primer and Topcoat for Genset - RAL 5010, gentian blue

	Spare Paint

	1
	Repair Paint - RAL 5010, gentian blue

	Name Plates for Complete Engine

	1
	Labeling of the genset - English (US)

	Genset Test

	1
	Genset acceptance test without customer participation

	Packing for Complete Genset

	1
	Packing suitable for overland transport for genset: foil cover

	Fuel System

	Zero-Pressure Gas Control Train

	Gas Train

	1
	Gas train DN 125/125 - with seal monitoring unit

	Connecting Accessories for Zero Pressure Train

	1
	Compensator for gasconnection

	Heating System

	Engine Cooling Circuit

	Lube Oil Heat Exchanger

	1
	Lube oil heat exchanger

	1
	Counter flange DN 100 - steel/stainless steel

	Sensors and Accessories

	1
	Gas and dirt separator DN 125

	1
	Counter Flange Set DN 125 - Set of 2

	Exhaust Gas System

	Sensors

	1
	Exhaust back pressure sensor

	Electrical System

	Genset Management (TEM)

	Base System

	1
	TEM - Basic Cabinet (ST32-F)

	1
	TEM packaging in wooden crate (VER)

	Power Plant Control System

	1
	Heat utilization with heating circuit (HK2)

	1
	Radiator controler (TKS1)

	1
	Acknowledgment of external monitoring (QEÜ)

	1
	Cabin air regulation (RL1)

	1
	Demand of external starting preparations (AES)

	1
	Handling of mains failure (NA)

	1
	Dump cooling and exhaust bypass control (NK/BY)











	Parameterizable Input/Output

	1
	2 parameterizable measurements (2MW)

	1
	1 parameterizable control circuit (1PR)

	Interface

	1
	Analog speed setting (ASD)

	1
	Remote Engine Management

	Hardware

	1
	I/O Controller (IOC) (included in Base system)

	1
	Operating terminal (BRT)

	1
	wall switch cabinet, Height 1200mm door hinge right (AE0R)

	1
	Console (KBW)

	1
	TEM connecting cable set 8m (K32ARM)

	Packing

	Plant Components

	1
	Packing plant components

	Documentation

	Documentation First language

	1
	Documentation first language - standard documentation

	1
	Data volume copy

	Documentation

	

	1
	Standard documentation incl. TEM documentation
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