|  |  |  |
| --- | --- | --- |
|  |  | **Estimated Price USD$** |
| **Startup/Commissioning Parts:** | Startup/commissioning parts are recommended to be available on site for immediate use during commissioning. Startup/commissioning parts typically include the following: spare fitting kit, hand tool kit, one (1) set of lube and fuel filtration elements, gaskets, O-rings, other sealing media, and a selection of electrical components with usage during normal startup and commissioning. | **$23,487.18** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Part Description** | **Recommended Qty** | **Unit Price** | **Ext Price** |
| **STARTUP/COMMISSIONING PARTS** |   |   |   |
| SEALANT, PIPE, PTFE  | 1 |  |  |
| LAMP, LED, RED,28 VDC  | 2 |  |  |
| INDICATOR, LIGHTED, YELLOW  | 1 |  |  |
| INDICATOR, LIGHTED, WHITE  | 10 |  |  |
| INDICATOR,LIGHTED,GREEN  | 2 |  |  |
| GASKET,SPIRAL,2.0,CL300,RF  | 2 |  |  |
| GASKET,SPIRAL,1.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,2.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,3.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,4.0,CL150,RF,304 | 2 |  |  |
| GASKET,SPIRAL,2.0,CL300,RF,304 | 2 |  |  |
| GASKET,0.375 OD,PFTE,JOINT  | 1 |  |  |
| SEAL,LIP  | 1 |  |  |
| HOLDER,FUSE  | 10 |  |  |
| FUSE,2 A  | 2 |  |  |
| FUSE,5 A  | 2 |  |  |
| FUSE,10 A  | 6 |  |  |
| FUSE,20 A  | 2 |  |  |
| FUSE,30 A  | 2 |  |  |
| CONNECTOR  | 2 |  |  |
| O-RING,NON-STD,31.625 ID,VITON | 1 |  |  |
| SENSOR,SPEED,ACTIVE  | 1 |  |  |
| KIT,ELEMENT,CARTRIDGE,PLEATED  | 1 |  |  |
| RELAY,DPDT,8 A  | 17 |  |  |
| SEAL,EXTRUSION  | 1 |  |  |
| KIT,ELEMENT,FILTER,LUBE OIL  | 2 |  |  |
| INDICATOR,LIGHTED  | 1 |  |  |
| KIT,ELEMENT,FILTER  | 2 |  |  |
| SEAL,METALLIC  | 1 |  |  |
| SOCKET,RELAY,24 VDC,10 A  | 1 |  |  |
| ELEMENT,BARRIER,CELLULOSE  | 1 |  |  |
| SET,BOLT,SHEAR  | 1 |  |  |
| ADHESIVE,THREADLOCK  | 2 |  |  |
| BOLT,HEX,0.375-16 X 1.0 IN,B7  | 20 |  |  |
| CABLE,IGNITION,84.0 IN  | 1 |  |  |
| GROMMET,0.965 OD  | 1 |  |  |
| GROMMET,0.965 OD  | 1 |  |  |
| GASKET, INJECTOR  | 12 |  |  |
| GASKET,8.8 ID,10.66 OD,0.06 IN | 1 |  |  |
| GASKET X 2.71IN,.062,BLUE-GARD | 1 |  |  |
| PACKING,OIL DRAIN  | 6 |  |  |
| GASKET,5.62 X 5.62IN,.030  | 3 |  |  |
| GASKET,3.32 ID,3.68 OD,0.049  | 5 |  |  |
| KIT,ELEMENT,FILTER,LUBE OIL  | 1 |  |  |
| KIT,ELEMENT,FUEL,LUBE OIL,8.2  | 1 |  |  |
| SENSOR,SPEED,PASSIVE  | 1 |  |  |
| GASKET,1.471 ID,1.754 OD,0.150 | 1 |  |  |
| TAPE,FOAM  | 50 |  |  |
| SEALANT,PIPE,PUTTY  | 1 |  |  |
| BULB FLUOR BI-PIN TUBE 36W  | 2 |  |  |
| GASKET,42.25 ID,53 OD  | 1 |  |  |
| O-RING,SAE 015,VITON  | 25 |  |  |
| O-RING,SAE 214,1.0 ID,VITON  | 25 |  |  |
| O-RING,SAE 227,2.125 ID,VITON  | 10 |  |  |
| O-RING,SAE 158,4.75 ID,VITON  | 6 |  |  |
| GASKET,0.77 ID,METALLIC,SPARK  | 25 |  |  |
| SPARK PLUG  | 2 |  |  |
| O-RING,SAE 166,6.75 ID,VITON  | 4 |  |  |
| O-RING,SAE 117,0.8125 ID,VITON | 25 |  |  |
| O-RING,SAE 225,1.875 ID,VITON  | 15 |  |  |
| O-RING,SAE 222,1.5 ID,VITON  | 25 |  |  |
| O-RING,SAE 932,2.337 ID,VITON  | 8 |  |  |
| O-RING,SAE 122,1.125 ID,VITON  | 25 |  |  |
| O-RING,SAE 924,1.72 ID,VITON  | 12 |  |  |
| LAMP,INCANDESCENT,CLEAR,28 VDC | 4 |  |  |
| SEAL,THREADED,0.625 ID,1.1875  | 8 |  |  |
| RESISTOR,0.25 W,10000 OHM  | 25 |  |  |
| SEAL,METALLIC  | 4 |  |  |
| WIRE,SAFETY,0.032 IN,302/304  | 1 |  |  |
| O-RING,SAE 224,1.75 ID,VITON  | 14 |  |  |
| SEAL,THREADED,0.375 ID,0.75 OD | 10 |  |  |
| O-RING,SAE 137,VITON  | 6 |  |  |
| SEAL,THREADED,0.759 ID,1.023  | 1 |  |  |
| BLOCK,MOUNTING,BARRIER SYS  | 12 |  |  |
| SEAL, METALLIC 1/4'' SAE O-RNG | 1 |  |  |
| SEAL,METALLIC  | 1 |  |  |
| SEAL,METALLIC  | 1 |  |  |
| GASKET 6'' 150# FULL FACE  | 1 |  |  |
| SEALANT  | 3 |  |  |
| KIT,TOOL,HAND  | 1 |  |  |
| TOOL,REPLACEMENT FITTINGS  | 1 |  |  |
| **Subtotal (STARTUP/COMMISSIONING PARTS)** |   |   | **$23,487.18** |